TTY_IOCTL(4)

NAME
tty ioctl - ioctls for terminals and serial lines

SYNOPSIS
#include <termios.h>

int ioctl(int fd, int cmd, ...);

DESCRIPTION
The ioctl() call for terminals and serial ports accepts many possible command arguments. Most require a third argument, of varying type, here called argp or arg.

Use of ioctl makes for non-portable programs. Use the POSIX interface described in termios(3) whenever possible.

  Get and Set Terminal Attributes

TCGETS	struct termios *argp
    Equivalent to tcgetattr(fd, argp).
    Get the current serial port settings.

TCSETS	const struct termios *argp
    Equivalent to tcsetattr(fd, TCSANOW, argp).
    Set the current serial port settings.

TCSETSW	const struct termios *argp
    Equivalent to tcsetattr(fd, TCSADRAIN, argp).
    Allow the output buffer to drain, and set the current serial port settings.

TCSETSF	const struct termios *argp
    Equivalent to tcsetattr(fd, TCSAFLUSH, argp).
    Allow the output buffer to drain, discard pending input, and set the current serial port settings.

The following four ioctls are just like TCGETS, TCSETS, TCSETSW, TCSETSF, except that they take a struct termio * instead of a struct termios *.

TCGETA	struct termio *argp

TCSETA	const struct termio *argp

TCSETAW	const struct termio *argp

TCSETAF	const struct termio *argp

  Locking the termios structure
The termios structure of a tty can be locked. The lock is itself a termios structure, with non-zero bits or fields indicating a locked value.

TIOCGLCKTRMIOS	struct termios *argp
    Gets the locking status of the termios structure of the terminal.

TIOCSLCKTRMIOS	const struct termios *argp
    Sets the locking status of the termios structure of the terminal. Only root can do this.

  Get and Set Window Size
Window sizes are kept in the kernel, but not used by the kernel (except in the case of virtual consoles, where the kernel will update the window size when the size of the virtual console changes, for example, by loading a new font). The following constants and structure are defined in <sys/ioctl.h>.

TIOCGWINSZ	struct winsize *argp
    Get window size.

TIOCSWINSZ	const struct winsize *argp
    Set window size.

The struct used by these ioctls is defined as
struct winsize {
    unsigned short ws_row;
    unsigned short ws_col;
    unsigned short ws_xpixel;   /* unused */
    unsigned short ws_ypixel;   /* unused */
};
When the window size changes, a SIGWINCH signal is sent to the foreground process group.

  Sending a Break

TCSBRK	int arg
    Equivalent to tcsendbreak(fd, arg).
    If the terminal is using asynchronous serial data transmission, and arg is zero, then send a break (a stream of zero bits) for between 0.25 and 0.5 seconds. If the terminal is not using asynchronous serial data transmission, then either a break is sent, or the function returns without doing anything. When arg is non-zero, nobody knows what will happen. (SVr4, UnixWare, Solaris, Linux treat tcsendbreak(fd,arg) with non-zero arg like tcdrain(fd). SunOS treats arg as a multiplier, and sends a stream of bits arg times as long as done for zero arg. DG/UX and AIX treat arg (when non-zero) as a timeinterval measured in milliseconds. HP-UX ignores arg.)

TCSBRKP	int arg
    So-called "POSIX version" of TCSBRK. It treats non-zero arg as a timeinterval measured in deciseconds, and does nothing when the driver does not support breaks.

TIOCSBRK	void
    Turn break on, that is, start sending zero bits.

TIOCCBRK	void
    Turn break off, that is, stop sending zero bits.

  Software flow control

TCXONC	int arg
    Equivalent to tcflow(fd, arg).
    See tcflow(3) for the argument values TCOOFF, TCOON, TCIOFF, TCION.

  Buffer count and flushing

FIONREAD	int *argp
    Get the number of bytes in the input buffer.

TIOCINQ	int *argp
    Same as FIONREAD.

TIOCOUTQ	int *argp
    Get the number of bytes in the output buffer.

TCFLSH	int arg
    Equivalent to tcflush(fd, arg).
    See tcflush(3) for the argument values TCIFLUSH, TCOFLUSH, TCIOFLUSH.

  Faking input

TIOCSTI	const char *argp
    Insert the given byte in the input queue.

  Redirecting console output

TIOCCONS	void
    Redirect output that would have gone to /dev/console or /dev/tty0 to the given tty. If that was a pty master, send it to the slave. Anybody can do this as long as the output was not redirected yet. If it was redirected already EBUSY is returned, but root may stop redirection by using this ioctl with fd pointing at /dev/console or /dev/tty0.

  Controlling tty

TIOCSCTTY	int arg
    Make the given tty the controlling tty of the calling process. The calling process must be a session leader and not have a controlling tty already. If this tty is already the controlling tty of a different session group then the ioctl fails with EPERM, unless the caller is root and arg equals 1, in which case the tty is stolen, and all processes that had it as controlling tty lose it.

TIOCNOTTY void
    If the given tty was the controlling tty of the calling process, give up this controlling tty. If the process was session leader, then send SIGHUP and SIGCONT to the foreground process group and all processes in the current session lose their controlling tty.

  Process group and session ID

TIOCGPGRP	pid_t *argp
    When successful, equivalent to *argp = tcgetpgrp(fd).
    Get the process group ID of the foreground process group on this tty.

TIOCSPGRP	const pid_t *argp
    Equivalent to tcsetpgrp(fd, *argp).
    Set the foreground process group ID of this tty.

TIOCGSID	pid_t *argp
    Get the session ID of the given tty. This will fail with ENOTTY in case the tty is not a master pty and not our controlling tty. Strange.

  Exclusive mode

TIOCEXCL	void
    Put the tty into exclusive mode. No further open(2) operations on the terminal are permitted. (They will fail with EBUSY, except for root.)

TIOCNXCL	void
    Disable exclusive mode.

  Line discipline

TIOCGETD	int *argp
    Get the line discipline of the tty.

TIOCSETD	const int *argp
    Set the line discipline of the tty.

  Pseudo-tty ioctls

TIOCPKT	const int *argp
    Enable (when *argp is non-zero) or disable packet mode. Can be applied to the master side of a pseudo-terminal only (and will return ENOTTY otherwise). In packet mode, each subsequent read(2) will return a packet that either contains a single non-zero control byte, or has a single byte containing zero (' ') followed by data written on the slave side of the pty. If the first byte is not TIOCPKT_DATA (0), it is an OR of one or more of the following bits:
    TIOCPKT_FLUSHREAD   The read queue for the terminal is flushed.
    TIOCPKT_FLUSHWRITE  The write queue for the terminal is flushed.
    TIOCPKT_STOP        Output to the terminal is stopped.
    TIOCPKT_START       Output to the terminal is restarted.
    TIOCPKT_DOSTOP      The start and stop characters are ^S/^Q.
    TIOCPKT_NOSTOP      The start and stop characters are not ^S/^Q.
    While this mode is in use, the presence of control status information to be read from the master side may be detected by a select(2) for exceptional conditions. This mode is used by rlogin(1) and rlogind(8) to implement a remote-echoed, locally ^S/^Q flow-controlled remote login. The BSD ioctls TIOCSTOP, TIOCSTART, TIOCUCNTL, TIOCREMOTE have not been implemented under Linux.

  Modem control

TIOCMGET	int *argp
    get the status of modem bits.

TIOCMSET	const int *argp
    set the status of modem bits.

TIOCMBIC	const int *argp
    clear the indicated modem bits.

TIOCMBIS	const int *argp
    set the indicated modem bits.

Bits used by these four ioctls:
TIOCM_LE        DSR (data set ready/line enable)
TIOCM_DTR       DTR (data terminal ready)
TIOCM_RTS       RTS (request to send)
TIOCM_ST        Secondary TXD (transmit)
TIOCM_SR        Secondary RXD (receive)
TIOCM_CTS       CTS (clear to send)
TIOCM_CAR       DCD (data carrier detect)
TIOCM_CD         see TIOCM_CAR
TIOCM_RNG       RNG (ring)
TIOCM_RI         see TIOCM_RNG
TIOCM_DSR       DSR (data set ready)

  Marking a line as local

TIOCGSOFTCAR	int *argp
    ("Get software carrier flag") Get the status of the CLOCAL flag in the c_cflag field of the termios structure.

TIOCSSOFTCAR	const int *argp
    ("Set software carrier flag") Set the CLOCAL flag in the termios structure when *argp is non-zero, and clear it otherwise.

If the CLOCAL flag for a line is off, the hardware carrier detect (DCD) signal is significant, and an open(2) of the corresponding tty will block until DCD is asserted, unless the O_NONBLOCK flag is given. If CLOCAL is set, the line behaves as if DCD is always asserted. The software carrier flag is usually turned on for local devices, and is off for lines with modems.

  Linux-specific
For the TIOCLINUX ioctl, see console_ioctl(4).

  Kernel debugging
#include <linux/tty.h>

TIOCTTYGSTRUCT	struct tty_struct *argp
    Get the tty_struct corresponding to fd.

RETURN VALUE
The ioctl() system call returns 0 on success. On error it returns -1 and sets errno appropriately.

ERRORS

EINVAL
    Invalid command parameter.

ENOIOCTLCMD
    Unknown command.

ENOTTY
    Inappropriate fd.

EPERM
    Insufficient permission.

EXAMPLE
Check the condition of DTR on the serial port.
#include <termios.h>
#include <fcntl.h>
#include <sys/ioctl.h>
int
main(void)
{
    int fd, serial;
    fd = open("/dev/ttyS0", O_RDONLY);
    ioctl(fd, TIOCMGET, &serial);
    if (serial & TIOCM_DTR)
        puts("TIOCM_DTR is not set");
    else
        puts("TIOCM_DTR is set");
    close(fd);
}

SEE ALSO
ioctl(2), termios(3), console_ioctl(4), pty(7)

COLOPHON
This page is part of release 3.05 of the Linux man-pages project. A description of the project, and information about reporting bugs, can be found at http://www.kernel.org/doc/man-pages/.