TRACEROUTE(8)

NAME
traceroute - print the route packets trace to network host

SYNOPSIS
traceroute [-46dFITUnrAV] [-f first_ttl] [-g gate,...]
[-i device] [-m max_ttl] [-p port] [-s src_addr]
[-q nqueries] [-N squeries] [-t tos]
[-l flow_label] [-w waittime] [-z sendwait]
[-UL] [-P proto] [--sport=port] [-M method] [-O mod_options]
host [packetlen]
traceroute6 [options]
tracert [options]
tcptraceroute [options]

DESCRIPTION
traceroute tracks the route packets taken from an IP network on their way to a given host. It utilizes the IP protocol's time to live (TTL) field and attempts to elicit an ICMP TIME_EXCEEDED response from each gateway along the path to the host.

traceroute6 is equivalent to traceroute -6
tracert is equivalent to traceroute -I
tcptraceroute is equivalent to traceroute -T

The only required parameter is the name or IP address of the destination host . This parameter can be followed by the size of the probing packet sent to that host (40 by default). Varying the size of the packet in conjunction with the -F parameter can be used to obtain information about the MTU of individual network hops. (The size parameter is useless for TCP probes).

This program attempts to trace the route an IP packet would follow to some internet host by launching probe packets with a small ttl (time to live) then listening for an ICMP "time exceeded" reply from a gateway. We start our probes with a ttl of one and increase by one until we get an ICMP "port unreachable" (or TCP reset), which means we got to the "host", or hit a max (which defaults to 30 hops). Three probes (by default) are sent at each ttl setting and a line is printed showing the ttl, address of the gateway and round trip time of each probe. If the probe answers come from different gateways, the address of each responding system will be printed. If there is no response within a 5.0 seconds (default), an "*" is printed for that probe.

After the trip time, some additional annotation can be printed: !H, !N, or !P (host, network or protocol unreachable), !S (source route failed), !F (fragmentation needed), !X (communication administratively prohibited), !V (host precedence violation), !C (precedence cutoff in effect), or !<num> (ICMP unreachable code <num>). If almost all the probes result in some kind of unreachable, traceroute will give up and exit.

We don't want the destination host to process the UDP probe packets, so the destination port is set to an unlikely value (you can change it with the -p flag). There is no such a problem for ICMP or TCP tracerouting (for TCP we use half-open technique, which prevents our probes to be seen by applications on the destination host).

In the modern network environment the traditional traceroute methods can not be always applicable, because of widespread use of firewalls. Such firewalls filter the "unlikely" UDP ports, or even ICMP echoes. To solve this, some additional tracerouting methods are implemented (including tcp), see LIST OF AVAILABLE METHODS below. Such methods try to use particular protocol and source/destination port, in order to bypass firewalls (to be seen by firewalls just as a start of allowed type of a network session).

OPTIONS

--help
    Print help info and exit.

-4, -6
    Explicitly force IPv4 or IPv6 traceouting. By default, the program will try to resolve the name given, and choose the appropriate protocol automatically. If resolving a host name returns both IPv4 and IPv6 addresses, traceroute will use IPv4.

-I  Use ICMP ECHO for probes

-T  Use TCP SYN for probes

-d  Enable socket level debugging (when the Linux kernel supports it)

-F  Set the "Don't Fragment" bit. This tells intermediate routers not to fragment the packet when they find it's too big for a network hop's MTU.

-f first_ttl
    Specifies with what TTL to start. Defaults to 1.

-g gateway
    Tells traceroute to add an IP source routing option to the outgoing packet that tells the network to route the packet through the specified gateway. Not very useful, because most routers have disabled source routing for security reasons.

-i interface
    Specifies the interface through which traceroute should send packets. By default, the interface is selected according to the routing table.

-m max_ttl
    Specifies the maximum number of hops (max time-to-live value) traceroute will probe. The default is 30.

-N squeries
    Specifies the number of probe packets sent out simultaneously. Sending several probes concurrently can speed up traceroute considerably. The default value is 16.
    Note that some routers and hosts can use ICMP rate throttling. In such a situation specifying too large number can lead to loss of some responses.

-n  Do not try to map IP addresses to host names when displaying them.

-p port
    For UDP tracing, specifies the destination port base traceroute will use (the destination port number will be incremented by each probe).
    For ICMP tracing, specifies the initial icmp sequence value (incremented by each probe too).
    For TCP specifies just the (constant) destination port to connect.

-t tos
    For IPv4, set the Type of Service (TOS) and Precedence value. Useful values are 16 (low delay) and 8 (high throughput). Note that in order to use some TOS precendence values, you have to be super user.
    For IPv6, set the Traffic Control value.

-w waittime
    Set the time (in seconds) to wait for a response to a probe (default 5.0 sec).

-q nqueries
    Sets the number of probe packets per hop. The default is 3.

-r  Bypass the normal routing tables and send directly to a host on an attached network. If the host is not on a directly-attached network, an error is returned. This option can be used to ping a local host through an interface that has no route through it.

-s source_addr
    Chooses an alternative source address. Note that you must select the address of one of the interfaces. By default, the address of the outgoing interface is used.

-z sendwait
    Minimal time interval between probes (default 0). If the value is more than 10, then it specifies a number in milliseconds, else it is a number of seconds (float point values allowed too). Useful when some routers use rate-limit for icmp messages.

-A  Perform AS path lookups in routing registries and print results directly after the corresponding addresses.

-V  Print the version and exit.

There is a couple of additional options, intended for an advanced usage (another trace methods etc.):

--sport=port
    Chooses the source port to use. Implies -N 1. Normally source ports (if applicable) are chosen by the system.

-M method
    Use specified method for traceroute operations. Default traditional udp method has name default, icmp (-I) and tcp (-T) have names icmp and tcp respectively.
    Method-specific options can be passed by -O . Most methods have their simple shortcuts, (-I means -M icmp, etc).

-O option
    Specifies some method-specific option. Several options are separated by comma (or use several -O on cmdline). Each method may have its own specific options, or many not have them at all. To print information about available options, use -O help.

-U  Use UDP to particular destination port for tracerouting (instead of increasing the port per each probe). Default port is 53 (dns).

-UL Use UDPLITE for tracerouting (default port is 53).

-P protocol
    Use raw packet of specified protocol for tracerouting. Default protocol is 253 (rfc3692).

LIST OF AVAILABLE METHODS
In general, a particular traceroute method may have to be chosen by -M name, but most of the methods have their simple cmdline switches (you can see them after the method name, if present).

  default
The traditional, ancient method of tracerouting. Used by default.

Probe packets are udp datagrams with so-called "unlikely" destination ports. The "unlikely" port of the first probe is 33434, then for each next probe it is incremented by one. Since the ports are expected to be unused, the destination host normally returns "icmp unreach port" as a final response. (Nobody knows what happens when some application listens for such ports, though).

This method is allowed for unprivileged users.

  icmp -I
Most usual method for now, which uses icmp echo packets for probes.
If you can ping(8) the destination host, icmp tracerouting is applicable as well.

  tcp -T
Well-known modern method, intended to bypass firewalls.
Uses the constant destination port (default is 80, http).

If some filters are present in the network path, then most probably any "unlikely" udp ports (as for default method) or even icmp echoes (as for icmp) are filtered, and whole tracerouting will just stop at such a firewall. To bypass a network filter, we have to use only allowed protocol/port combinations. If we trace for some, say, mailserver, then more likely -T -p 25 can reach it, even when -I can not.

This method uses well-known "half-open technique", which prevents applications on the destination host from seeing our probes at all. Normally, a tcp syn is sent. For non-listened ports we receive tcp reset, and all is done. For active listening ports we receive tcp syn+ack, but answer by tcp reset (instead of expected tcp ack), this way the remote tcp session is dropped even without the application ever taking notice.

There is a couple of options for tcp method:

syn,ack,fin,rst,psh,urg,ece,cwr
    Sets specified tcp flags for probe packet, in any combination.

flags=num
    Sets the flags field in the tcp header exactly to num.

ecn Send syn packet with tcp flags ECE and CWR (for Explicit Congestion Notification, rfc3168)

sack,timestamps,window_scaling
    Use the corresponding tcp header option in the outgoing probe packet.

sysctl
    Use current sysctl (/proc/sys/net/*) setting for the tcp header options above and ecn. Always set by default, if nothing else specified.

mss=num
    Use value of num for maxseg tcp header option (when syn).

Default options is syn,sysctl.

  tcpconn
An initial implementation of tcp method, simple using connect(2) call, which does full tcp session opening. Not recommended for normal use, because a destination application is always affected (and can be confused).

  udp -U
Use udp datagram with constant destination port (default 53, dns).
Intended to bypass firewall as well.

Note, that unlike in tcp method, the correspond application on the destination host always receive our probes (with random data), and most can easily be confused by them. Most cases it will not respond to our packets though, so we will never see the final hop in the trace. (Fortunately, it seems that at least dns servers replies with something angry).

This method is allowed for unprivileged users.

  udplite -UL
Use udplite datagram for probes (with constant destination port, default 53).

This method is allowed for unprivileged users.
Options:

coverage=num
    Set udplite send coverage to num.

  raw -P proto
Send raw packet of protocol proto.
No protocol-specific headers are used, just IP header only.
Implies -N 1.
Options:

protocol=proto
    Use IP protocol proto (default 253).

NOTES

To speed up work, normally several probes are sent simultaneously. On the other hand, it creates a "storm of packages", especially in the reply direction. Routers can throttle the rate of icmp responses, and some of replies can be lost. To avoid this, decrease the number of simultaneous probes, or even set it to 1 (like in initial traceroute implementation), i.e. -N 1

The final (target) host can drop some of the simultaneous probes, and might even answer only the latest ones. It can lead to extra "looks like expired" hops near the final hop. We use a smart algorithm to auto-detect such a situation, but if it cannot help in your case, just use -N 1 too.

For even greater stability you can slow down the program's work by -z option, for example use -z 0.5 for half-second pause between probes.

If some hops report nothing for every method, the last chance to obtain something is to use ping -R command (IPv4, and for nearest 8 hops only).

SEE ALSO
ping(8), ping6(8), tracepath(8), netstat(8)