KEYMAPS(5)

NAME
keymaps - keyboard table descriptions for loadkeys and dumpkeys

DESCRIPTION
These files are used by loadkeys(1) to modify the translation tables used by the kernel keyboard driver and generated by dumpkeys(1) from those translation tables. The format of these files is vaguely similar to the one accepted by xmodmap(1). The file consists of charset or key or string definition lines interspersed with comments. Comments are introduced with ! or # characters and continue to the end of the line. Anything following one of these characters on that line is ignored. Note that comments need not begin from column one as with xmodmap(1). The syntax of keymap files is line oriented; a complete definition must fit on a single logical line. Logical lines can, however, be split into multiple physical lines by ending each subline with the backslash character (\).

INCLUDE FILES
A keymap can include other keymaps using the syntax

    include "pathname"

CHARSET DEFINITIONS
A character set definition line is of the form:
    charset <charset>
Where <charset> is one of the currently supported charsets, which can be found using dumpkeys --help. It defines how following keysyms are to be interpreted. For example, in iso-8859-1 the symbol mu (or micro) has code 0265, while in iso-8859-7 the letter mu has code 0354.

COMPLETE KEYCODE DEFINITIONS
Each complete key definition line is of the form:
    keycode keynumber = keysym keysym keysym...
keynumber is the internal identification number of the key, roughly equivalent to the scan code of it. keynumber can be given in decimal, octal or hexadecimal notation. Octal is denoted by a leading zero and hexadecimal by the prefix 0x. Each of the keysyms represent keyboard actions, of which up to 256 can be bound to a single key. The actions available include outputting Latin1 character codes or character sequences, switching consoles or keymaps, booting the machine etc. (The complete list can be obtained from dumpkeys(1) by saying dumpkeys -l). Each keysym may be prefixed by a '+' (plus sign), in which case this keysym is treated as a "letter" and therefore affected by the "CapsLock" the same way as by "Shift" (to be correct, the CapsLock inverts the Shift state). The ASCII letters ('a'-'z' and 'A'-'Z') are made CapsLock'able by default. If Shift+CapsLock should not produce a lower case symbol, put lines like
    keycode 30 = +a A
in the map file. Which of the actions bound to a given key is taken when it is pressed depends on what modifiers are in effect at that moment. The keyboard driver supports 8 modifiers. These modifiers are labeled (completely arbitrarily) Shift, AltGr, Control, Alt, ShiftL, ShiftR, CtrlL and CtrlR. Each of these modifiers has an associated weight of power of two according to the following table:

    modifier
        weight

    Shift
          1
    AltGr
          2
    Control
          4
    Alt
          8
    ShiftL
         16
    ShiftR
         32
    CtrlL
         64
    CtrlR
        128
The effective action of a key is found out by adding up the weights of all the modifiers in effect. By default, no modifiers are in effect, so action number zero, i.e. the one in the first column in a key definition line, is taken when the key is pressed or released. When e.g. Shift and Alt modifiers are in effect, action number nine (from the 10th column) is the effective one.

Changing the state of what modifiers are in effect can be achieved by binding appropriate key actions to desired keys. For example, binding the symbol Shift to a key sets the Shift modifier in effect when that key is pressed and cancels the effect of that modifier when the key is released. Binding AltGr_Lock to a key sets AltGr in effect when the key is pressed and cancels the effect when the key is pressed again. (By default Shift, AltGr, Control and Alt are bound to the keys that bear a similar label; AltGr may denote the right Alt key.)

Note that you should be very careful when binding the modifier keys, otherwise you can end up with an unusable keyboard mapping. If you for example define a key to have Control in its first column and leave the rest of the columns to be VoidSymbols, you're in trouble. This is because pressing the key puts Control modifier in effect and the following actions are looked up from the fifth column (see the table above). So, when you release the key, the action from the fifth column is taken. It has VoidSymbol in it, so nothing happens. This means that the Control modifier is still in effect, although you have released the key. Re-pressing and releasing the key has no effect. To avoid this, you should always define all the columns to have the same modifier symbol. There is a handy short-hand notation for this, see below. keysyms can be given in decimal, octal, hexadecimal or symbolic notation. The numeric notations use the same format as with keynumber. The symbolic notation resembles that used by xmodmap(1). Notable differences are the number symbols. The numeric symbols '0', ..., '9' of xmodmap(1) are replaced with the corresponding words 'zero', 'one', ... 'nine' to avoid confusion with the numeric notation. It should be noted that using numeric notation for the keysyms is highly unportable as the key action numbers may vary from one kernel version to another and the use of numeric notations is thus strongly discouraged. They are intended to be used only when you know there is a supported keyboard action in your kernel for which your current version of loadkeys(1) has no symbolic name. If you do need to use numeric notations, comment those lines heavily and add a comment at the top of the file. This will save your sanity (if any) later. If this file should happen to get past your personal system, it may also save you much pain and embarrassment. Also, please file a bug report against loadkeys noting the need for a symbolic name. There is a number of short-hand notations to add readability and reduce typing work and the probability of typing-errors. First of all, you can give a map specification line, of the form
    keymaps 0-2,4-5,8,12
to indicate that the lines of the keymap will not specify all 256 columns, but only the indicated ones. (In the example: only the plain, Shift, AltGr, Control, Control+Shift, Alt and Control+Alt maps, that is, 7 columns instead of 256.) When no such line is given, the keymaps 0-M will be defined, where M+1 is the maximum number of entries found in any definition line. Next, you can leave off any trailing VoidSymbol entries from a key definition line. VoidSymbol denotes a keyboard action which produces no output and has no other effects either. For example, to define key number 30 to output 'a' unshifted, 'A' when pressed with Shift and do nothing when pressed with AltGr or other modifiers, you can write
    keycode 30 = a A
instead of the more verbose
    keycode 30 = a	A	VoidSymbol	VoidSymbol \
    		VoidSymbol VoidSymbol VoidSymbol ...
For added convenience, you can usually get off with still more terse definitions. If you enter a key definition line with only and exactly one action code after the equals sign, it has a special meaning. If the code (numeric or symbolic) is not an ASCII letter, it means the code is implicitly replicated through all columns being defined. If, on the other hand, the action code is an ASCII character in the range 'a', ..., 'z' or 'A', ..., 'Z' in the ASCII collating sequence, the following definitions are made for the different modifier combinations, provided these are actually being defined. (The table lists the two possible cases: either the single action code is a lower case letter, denoted by 'x' or an upper case letter, denoted by 'Y'.)

    modifier
        symbol

    none
        x    Y
    Shift
        X    y
    AltGr
        x    Y
    Shift+AltGr
        X    y
    Control
        Control_x    Control_y
    Shift+Control
        Control_x    Control_y
    AltGr+Control
        Control_x    Control_y
    Shift+AltGr+Control
        Control_x    Control_y
    Alt
        Meta_x    Meta_Y
    Shift+Alt
        Meta_X    Meta_y
    AltGr+Alt
        Meta_x    Meta_Y
    Shift+AltGr+Alt
        Meta_X    Meta_y
    Control+Alt
        Meta_Control_x    Meta_Control_y
    Shift+Control+Alt
        Meta_Control_x    Meta_Control_y
    AltGr+Control+Alt
        Meta_Control_x    Meta_Control_y
    Shift+AltGr+Control+Alt
        Meta_Control_x    Meta_Control_y

SINGLE MODIFIER DEFINITIONS
All the previous forms of key definition lines always define all the M+1 possible modifier combinations being defined, whether the line actually contains that many action codes or not. There is, however, a variation of the definition syntax for defining only single actions to a particular modifier combination of a key. This is especially useful, if you load a keymap which doesn't match your needs in only some modifier combinations, like AltGr+function keys. You can then make a small local file redefining only those modifier combinations and loading it after the main file. The syntax of this form is: { plain | <modifier sequence> } keycode keynumber = keysym

e.g.,
    plain keycode 14 = BackSpace
    control alt keycode 83 = Boot
    alt keycode 105 = Decr_Console
    alt keycode 106 = Incr_Console
Using "plain" will define only the base entry of a key (i.e. the one with no modifiers in effect) without affecting the bindings of other modifier combinations of that key.

STRING DEFINITIONS
In addition to comments and key definition lines, the keymap files can contain string definitions. These are used to define what each function key action code sends. The syntax of string definitions is:
    string keysym = text
text can contain literal characters, octal character codes in the format of backslash followed by up to three octal digits, and the three escape sequences \n, \\, and \", for newline, backslash and quote, respectively.

COMPOSE DEFINITIONS
Then there may also be compose definitions. They have syntax

    compose 'char' 'char' to 'char'
and describe how two bytes are combined to form a third one (when a dead accent or compose key is used). This is used to get accented letters and the like on a standard keyboard.

ABBREVIATIONS
Various abbreviations can be used with kbd-0.96 and later.

strings as usual
    Defines the usual values of the strings (but not the keys they are bound to).

compose as usual for "iso-8859-1"
    Defines the usual compose combinations.

alt_is_meta
    Whenever some combination is defined as an ASCII symbol, and there is a corresponding Alt keymap, define by default the corresponding Alt combination as Meta_value.

To find out what keysyms there are available for use in keymaps files, use the command
    dumpkeys --long-info
Unfortunately, there is currently no description of what each symbol does. It has to be guessed from the name or figured out from the kernel sources.

EXAMPLES
(Be careful to use a keymaps line, like the first line of `dumpkeys`, or "keymaps 0-15" or so.) The following entry exchanges the left Control key and the Caps Lock key on the keyboard:
    keycode  58 = Control
    keycode  29 = Caps_Lock
Key number 58 is normally the Caps Lock key, and key number 29 is normally the Control key. The following entry sets the Shift and Caps Lock keys to behave more nicely, like in older typewriters. That is, pressing Caps Lock key once or more sets the keyboard in CapsLock state and pressing either of the Shift keys releases it.
    keycode  42 = Uncaps_Shift
    keycode  54 = Uncaps_Shift
    keycode  58 = Caps_On
The following entry sets the layout of the edit pad in the enhanced keyboard to be more like that in the VT200 series terminals:
    keycode 102 = Insert
    keycode 104 = Remove
    keycode 107 = Prior
    shift keycode 107 = Scroll_Backward
    keycode 110 = Find
    keycode 111 = Select
    control alt   keycode 111 = Boot
    control altgr keycode 111 = Boot
Here's an example to bind the string "du\ndf\n" to the key AltGr-D. We use the "spare" action code F100 not normally bound to any key.
    altgr keycode 32 = F100
    string F100 = "du\ndf\n"

SEE ALSO
loadkeys(1), dumpkeys(1), showkey(1), xmodmap(1).